
SDDOT TYPE D
Description: Urban turf grass mix used on boulevards and turf areas where salt tolerance may be required.


PRODUCT OVERVIEW
Description: Urban turf grass mix used on boulevards and turf areas where salt tolerance may be required.
MIXTURE HIGHLIGHTS
▸  Blended and certified at our MCIA-approved facility to meet or exceed project specifications
▸  All seed labeled and packaged per Federal Seed Act and applicable state seed laws
▸  Purity and germination values certified per AOSA/ISTA laboratory standards

SPECIES COMPOSITION — BY WEIGHT
Description: Urban turf grass mix used on boulevards and turf areas where salt tolerance may be required.  Seeding Rate: 7.0 PLS lb / 1000 sq-ft  |
	Common Name
	Scientific Name
	PLS lb / 1000 sq-ft

	Kentucky Bluegrass
	Poa pratensis
	1.4

	Perennial Ryegrass
	Lolium perenne
	1.4

	Creeping Red Fescue
	Festuca rubra
	1.4

	Chewings Fescue
	Festuca rubra commutata
	1.4

	Alkali Grass
	Puccinellia distans
	1.4

	Total
	
	7.0


SEEDING RATES
	Seeding Rate
	7.0 PLS lb / 1000 sq-ft


CERTIFICATION & COMPLIANCE
	Seed Quality Certification
✓  MCIA-Approved Seed Blending Facility — licensed to mix, bag, and distribute
✓  All seed labeled and packaged per Federal Seed Act (7 CFR Part 201)
✓  Minnesota Seed Law (Minn. Stat. §21) compliant in state of sale
✓  Germination tested per AOSA/ISTA laboratory standards
✓  Seed test date confirmed within 9 months of test date
✓  Lot numbers consistent across all tags, analysis reports, and shipping records
✓  Lot-specific seed analysis and tags available upon request with each order



	Certification Tag Reference
✓  Certified class cultivars used where available
✓  Seed analysis reports (one per lot) included with shipment
✓  Blend data sheet available per MCIA conditioning records



MANUFACTURER CERTIFICATION
	Ramy Turf Products certifies that the SDDOT TYPE D seed mixture described herein has been blended and tested in accordance with all applicable federal and state seed laws, accepted industry standards, and the requirements of applicable project specifications. All purity, germination, and weed content values reflect current laboratory analysis records on file at our MCIA-approved facility. Seed lot numbers, analysis reports, and certification tags will be provided with each shipment or upon request.
Like or better cultivars may be used based on availability and market conditions. Current substitution documentation and supporting records are available upon request. Please allow 3–5 business days for production. Custom and native mixtures are final sale once produced.



	Michael Ramy,  Owner — Ramy Turf Products
MCIA Approved Seed Blending Facility
	  
	Date



Full product details available at:  ramyturf.com/product/sddot-type-d     Questions?  info@ramyturf.com  |  800-658-RAMY
