
IOWA SUDAS TYPE 4 – URBAN TEMPORARY EROSION MIX
Short-term stabilization (6–8 months)


PRODUCT OVERVIEW
Temporary erosion control mix designed for rapid establishment and seasonal flexibility.
MIXTURE HIGHLIGHTS
▸  Blended and certified at our MCIA-approved facility to meet or exceed project specifications
▸  All seed labeled and packaged per Federal Seed Act and applicable state seed laws
▸  Purity and germination values certified per AOSA/ISTA laboratory standards
SPECIES COMPOSITION — BY WEIGHT
Iowa SUDAS Type 4 – Urban Temporary Erosion Mix
	Season
	Species
	Rate (lb/acre)

	Spring
	Annual Ryegrass
	40

	Spring
	Oats
	65

	Summer
	Annual Ryegrass
	50

	Summer
	Oats
	95

	Fall
	Annual Ryegrass
	40

	Fall
	Grain Rye
	65


CERTIFICATION & COMPLIANCE
	Seed Quality Certification
✓  MCIA-Approved Seed Blending Facility — licensed to mix, bag, and distribute
✓  All seed labeled and packaged per Federal Seed Act (7 CFR Part 201)
✓  Germination tested per AOSA/ISTA laboratory standards
✓  Seed test date confirmed within 12 months of test date
✓  Lot numbers consistent across all tags, analysis reports, and shipping records
✓  Lot-specific seed analysis and tags available upon request with each order



	Certification Tag Reference
✓  Certified class cultivars used where available
✓  Seed analysis reports (one per lot) included with shipment
✓  Blend data sheet available per MCIA conditioning records



MANUFACTURER CERTIFICATION
	Ramy Turf Products certifies that the IOWA SUDAS TYPE 4 – URBAN TEMPORARY EROSION MIX seed mixture described herein has been blended and tested in accordance with all applicable federal and state seed laws, accepted industry standards, and the requirements of applicable project specifications. All purity, germination, and weed content values reflect current laboratory analysis records on file at our MCIA-approved facility. Seed lot numbers, analysis reports, and certification tags will be provided with each shipment or upon request.
Like or better cultivars may be used based on availability and market conditions. Current substitution documentation and supporting records are available upon request. Please allow 3–5 business days for production. Custom and native mixtures are final sale once produced.



	Michael Ramy,  Owner — Ramy Turf Products
MCIA Approved Seed Blending Facility
	  
	Date



Full product details available at:  ramyturf.com/product/iowa-sudas-type-4-urban-temporary-erosion-mix     Questions?  info@ramyturf.com  |  800-658-RAMY
