
SEED MIXTURE SUBMITTAL / TECHNICAL DATA
STREET SIDE – BOULEVARD SALT TOLERANT


PRODUCT OVERVIEW
Street Side is engineered for boulevard, median, and roadside applications exposed to deicing salts, vehicle spray, compaction, and freeze-thaw cycles. The blend combines alkali grass with improved cool-season turf species to provide structural density, salt tolerance, and long-term performance in high-stress urban corridors.  SPECIES COMPOSITION (BY WEIGHT)  | Common Name | Scientific Name | % of Mix | | --- | --- | --- | | Alkali Grass (Salt-Tolerant Selection) | Puccinellia distans | 25% | | Kentucky Bluegrass (Improved Selection) | Poa pratensis | 25% | | Perennial Ryegrass (Improved Turf-Type) | Lolium perenne | 20% | | Chewings Fescue (Improved Fine Fescue) | Festuca rubra ssp. commutata | 15% | | Creeping Red Fescue (Improved Selection) | Festuca rubra | 15% |
MIXTURE HIGHLIGHTS
▸  Blended and certified at our MCIA-approved facility to meet or exceed project specifications
▸  All seed labeled and packaged per Federal Seed Act and applicable state seed laws
▸  Purity and germination values certified per AOSA/ISTA laboratory standards

SPECIES COMPOSITION — BY WEIGHT
SEED MIXTURE SUBMITTAL / TECHNICAL DATA
	Common Name
	Scientific Name
	% of Mix

	Alkali Grass (Salt-Tolerant Selection)
	Puccinellia distans
	25%

	Kentucky Bluegrass (Improved Selection)
	Poa pratensis
	25%

	Perennial Ryegrass (Improved Turf-Type)
	Lolium perenne
	20%

	Chewings Fescue (Improved Fine Fescue)
	Festuca rubra ssp. commutata
	15%

	Creeping Red Fescue (Improved Selection)
	Festuca rubra
	15%



STREET SIDE – BOULEVARD SALT TOLERANT
SEEDING RATES
	New Seeding
	5–6 lbs per 1,000 sq ft (approximately 220–260 lbs per acre).

	Overseeding
	3–4 lbs per 1,000 sq ft (approximately 130–175 lbs per acre).


MAINTENANCE PROFILE
	Maintenance Level
	Moderate

	Water Requirement
	1–1.5 inches per week (adjust based on salt exposure).

	Fertilizer Applications
	3–4 per year, particularly formulations suited for salt-affected soils.

	Suggested Mowing Height
	2–3 inches.


Full product details available at:  ramyturf.com/product/street-side/  Questions? Contact info@ramyturf.com  Ramy Turf Products | ramyturf.com | 800-658-RAMY  Ramy Turf Products is an MCIA-approved seed blending facility licensed to mix, bag, and distribute seed mixtures for federal, state, municipal, and private projects. All seed is labeled and packaged in full compliance with applicable federal and state seed laws and specification requirements in the state of sale. Like or better cultivars may be used based on availability and market conditions. Current substitution documentation and supporting records are available upon request. Please allow 3–5 business days for production of custom and native seed mixtures. Custom and native seed mixtures are blended specifically to order and, once produced, are considered final sale and not eligible for return.  For additional information, please contact Michael Ramy at 651-917-0939.  Michael Ramy Owner Ramy Turf Products MCIA Approved Seed Blending Facility Phone: 651-917-0939  Date:2/23/2026
CERTIFICATION & COMPLIANCE
	Seed Quality Certification
✓  MCIA-Approved Seed Blending Facility — licensed to mix, bag, and distribute
✓  All seed labeled and packaged per Federal Seed Act (7 CFR Part 201)
✓  Minnesota Seed Law (Minn. Stat. §21) compliant in state of sale
✓  Purity ≥ 98% guaranteed on all components
✓  Germination tested per AOSA/ISTA laboratory standards
✓  Seed test date confirmed within 15 months of test date
✓  Lot numbers consistent across all tags, analysis reports, and shipping records
✓  Lot-specific seed analysis and tags available upon request with each order



	Certification Tag Reference
✓  Certified class cultivars used where available
✓  Seed analysis reports (one per lot) included with shipment
✓  Blend data sheet available per MCIA conditioning records



MANUFACTURER CERTIFICATION
	Ramy Turf Products certifies that the SEED MIXTURE SUBMITTAL / TECHNICAL DATA seed mixture described herein has been blended and tested in accordance with all applicable federal and state seed laws, accepted industry standards, and the requirements of applicable project specifications. All purity, germination, and weed content values reflect current laboratory analysis records on file at our MCIA-approved facility. Seed lot numbers, analysis reports, and certification tags will be provided with each shipment or upon request.
Like or better cultivars may be used based on availability and market conditions. Current substitution documentation and supporting records are available upon request. Please allow 3–5 business days for production. Custom and native mixtures are final sale once produced.



	Michael Ramy,  Owner — Ramy Turf Products
MCIA Approved Seed Blending Facility
	  
	Date



Full product details available at:  ramyturf.com/product/seed-mixture-submittal-technical-data     Questions?  info@ramyturf.com  |  800-658-RAMY
